***NISSAN PATROL CRD EGR DELETE***

Tools Needed

* Socket set
* Screw driver
* Brake cleaner

Part 1.

Pull engine cover and Intercooler off

Unplug the Map sensor carefully please



Part 2.

Undo the 2x 12mm bolts that are marked in white




Part 3.

Undo the 2x 12mm bolts on the EGR flange



Part 4.


Manipulate the pipe a little to give you some room to pull the gasket out and slide the EGR plate in.



Once you have put the plate in you can now put the 2x 12mm bolts but into the flange

You can now put the 2x 12mm bolts back onto the EGR cooler

PHOTO IN NEXT PAGE



Part 5.

Clean the intercooler pipes where the cooler fits into

Clean the intercooler pipe end



this will stop the pipe from coming off

Part 6.

Fit engine cover but onto car



Part 7.

Fit the Supplied wiring loom onto the Maf sensor on the airbox



Now you are all done

Start the car and check for engine lights

Any questions please call

(07) 49530040

Facebook

Diesel Smart Performance Products

[www.dieselsmart.com.au](http://www.dieselsmart.com.au)

Thanks For your Business